{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["LuK Standard-Mehrweg-Packmittel"],"not_rendered":{"charts":0,"images":14,"macros":1,"external_links":0,"defined_names":5,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"LuK Standard-Mehrweg-Packmittel","index":0,"n_rows":16,"n_cols":15,"rows_kept":16,"cut":false,"hidden":false,"merged":[[2,0,2,14],[1,0,1,14],[0,0,0,14]]}
[]
["Standard-Mehrweg-Packmittel zur Belieferung der LuK Werke"]
["Standard-Reusable-Packaging for delivery to LuK plants"]
["Materialnr.","Foto ","Kurzzeichen ","Bezeichnung",null,"Verwendung:\nW = werksintern\nL = Lieferanten\nI =Intercompany","Bemerkung",null,"Gewicht  \n[kg]","Länge aussen \n[mm]","Breite aussen \n[mm]","Höhe aussen \n[mm]","Länge innen \n[mm]","Breite innen \n[mm]","Höhe innen \n[mm]"]
["materialno.","photo","short mark",null,"description","application:\nW = in-plant\nL = supplier\nI =Intercompany",null,"remark","weight \n[kg]","length external\n[mm]","width external\n[mm]","height external\n[mm]","length internal\n[mm]","width internal\n[mm]","height internal\n[mm]"]
["049900021-0000",null,"GP-KL_1","LUK-KLAPPGITTERBOX HOCH","LUK COLLAPSIABLE","W / L / I",null,null,86.8,1220,824,960,1140,744,764]
["051049031-0000",null,"GP-KL_2","LUK-KLAPPGITTERBOX NIEDRIG","LUK-KLAPPGITTERBOX NIEDRIG","W / L / I",null,null,74,1220,824,670,1140,744,432]
["058188630-0000",null,"K1208","SCHAEFFLER-KLAPPSTAHLBEHÄLTER 1200x800","SCHAEFFLER-KLAPPSTAHLBEHÄLTER 1200x800","W / L / I",null,null,98,1200,800,650,1150,740,480]
["002439140-0000",null,"EURO-FLP","EURO-PALETTE","EURO-PALETTE","W / L / I","entfällt mittelfristig","intermediate-term no longer applicable",25,1200,800,145,"-","-","-"]
["011023031-0000",null,"K-PAL_1","SCHAEFFLER-KUNSTSTOFFPALETTE SCHWARZ","SCHAEFFLER-KUNSTSTOFFPALETTE SCHWARZ","W / L / I",null,null,18,1200,800,160,"-","-","-"]
["071482997-0000",null,"KLT 3215","SCHAEFFLER-KLT 3215","SCHAEFFLER-KLT 3215","W / L / I",null,null,0.56999999999999995,300,200,147,243,163,129.5]
["070553300-0000",null,"KLT 4315","SCHAEFFLER-KLT 4315","SCHAEFFLER-KLT 4315","W / L / I",null,null,1.29,400,300,147,346,265,109.5]
["071483390-0000",null,"KLT 6415","SCHAEFFLER-KLT 6415","SCHAEFFLER-KLT 6415","W / L / I",null,null,2.2000000000000002,600,400,147,544,364,109.5]
["050886320-0000",null,"KLT 4328","SCHAEFFLER-KLT 4328","SCHAEFFLER-KLT 4328","W / L / I",null,null,2.6,400,300,280,334,247,236]
["073713317-0000",null,"KLT 6429","SCHAEFFLER-KLT 6429","SCHAEFFLER-KLT 6429","W / L / I",null,null,2.97,600,400,280,544,364,242]
["079981771-0000",null,"A 1208","SCHAEFFLER ABDECKPLATTE A1208","SCHAEFFLER COVERING PLATE 1208","W / L / I",null,null,5.15,1200,800,94,"-","-","-"]